Die Zeilen mit zwei Ausrufezeichen sind besondere Zeilen. Diese markieren neue Abschnitte in der Datei.
Diese Zeilen müssen am Anfang einer Zeile stehen und dürfen keine Leerzeichen beinhalten.
Darüberhinaus sind alle Zeichen groß zu schreiben.

Als erstes muss !!ROUTER kommen, diese Zeile markiert den eigentlichen Anfang. Es passiert nichts bis !!VARIABLEN erscheint.
Ab dort erfolgt die Definition der Variablen.

Ab !!CONFIG kommt die eigentliche Konfiguration. Alle im Abschnitt !!VARIABLEN definierten Werte werden im Abschnitt !!CONFIG eingesetzt.

Ansonsten sind Zeilen die mit einem ! beginnen Kommentare (Cisco Syntax).

!!ROUTER

!!VARIABLEN

<HOSTNAME>		=	R6
<TFTP_HOST_STRING>	=	tftp://172.23.210.222/x-confg

<INT_NAME>		=	f0/0
!<INT_IP_MASK>		=	192.1.1.2 255.255.255.0
<INT_IP_MASK>		=	DHCP

<DEF_GW>		=	

<SNMP_READ>		=	con
<SNMP_WRITE>		=	5NMP-Wr1t3-(0mm

<SYSLOG_FACILITY>	=	local1
<SYSLOG_SRC_INT>	=	
<SYSLOG_SEVERITY>	=	errors
<SYSLOG_SRV>		=	10.101.0.11
<LOG_SEVERITY>		=	informational


<SOMMERZEITVONBIS>	= Mar 31 2013 2:00 Oct 27 2013 2:00
<NTP_SRV1>		=	90.200.31.21
<NTP_SRV2>		=	90.200.31.23

! PTB NTP Server
! ntp server 192.53.103.103
! ntp server 192.53.103.108
! ntp server 192.53.103.104


<DOMAIN>		=	corp.conet.local
<ADM_PW>		=	LicherExport

! Netze/IPs zur Administration, AdminText, AdminNetz
<AT1>		=	extern 1
<AN1>		=	195.20.133.6
<AT2>		=	extern 2
<AN2>		=	212.202.166.58
<AT3>		=	Eschborner Ldstr 1
<AN3>		=	192.168.88.0 0.0.0.255
<AT4>		=	Eschborner Ldstr 2
<AN4>		=	172.23.210.0 0.0.0.255
<AT5>		=	Interxion
<AN5>		=	88.205.102.128 0.0.0.127
<ATI>		=	Initial Netz
<ANI>		=	192.1.1.0 0.0.0.255


!!CONFIG

boot network <TFTP_HOST_STRING>

hostname <HOSTNAME>

int <INT_NAME>
 ip address <INT_IP_MASK>
 no shut


ip route 0.0.0.0 0.0.0.0 <DEF_GW>

! snmp
snmp-server community <SNMP_READ> RO ACL_telnet_ssh_snmp
snmp-server community <SNMP_WRITE> RW ACL_telnet_ssh_snmp


! syslog
logging facility <SYSLOG_FACILITY>
logging source-interface <SYSLOG_SRC_INT>
logging <SYSLOG_SRV>
logging trap <SYSLOG_SEVERITY>

! lokales log
logging buffered 4096 <LOG_SEVERITY>
logging history <LOG_SEVERITY>
logging console <LOG_SEVERITY>
logging monitor <LOG_SEVERITY>


! ntp
clock timezone MEZ 1
clock summer-time MESZ date <SOMMERZEITVONBIS>

ntp server <NTP_SRV1> prefer
ntp server <NTP_SRV2>

! ssh
ip domain name <DOMAIN>
!crypto key generate rsa
!1024
!ip ssh ver 2
username admin priv 15 pass <ADM_PW>


! login
ip access-list standard ACL_telnet_ssh_snmp
remark <AT1>
permit <AN1>
remark <AT2>
permit <AN2>
remark <AT3>
permit <AN3>
remark <AT4>
permit <AN4>
remark <AT5>
permit <AN5>
remark <ATI>
permit <ANI>


line vty 0 4
 session-timeout 60
 access-class ACL_telnet_ssh_snmp in
 exec-timeout 60 0
 login local
 transport input all
line con 0
 login local
line aux 0
 login local


! services
service tcp-keepalives-in
service timestamps debug datetime localtime show-timezone
service timestamps log datetime localtime show-timezone
service password-encryption
service linenumber


! domain-lookup
no ip domain-lookup


! http
no ip http server


end
