
!
version 12.4
service tcp-keepalives-in
service timestamps debug datetime localtime show-timezone
service timestamps log datetime localtime show-timezone
service password-encryption
service linenumber
!
hostname R6
!
boot-start-marker
boot network tftp://172.23.210.222/x-confg
boot-end-marker
!
logging buffered 4096 informational
logging console informational
logging monitor informational
!
no aaa new-model
!
resource policy
!
clock timezone MEZ 1
clock summer-time MESZ date Mar 31 2013 2:00 Oct 27 2013 2:00
ip cef
!
!
!
!
no ip domain lookup
ip domain name corp.conet.local
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
username admin privilege 15 password 7 00281A050C5E19231731435C1D
!
! 
!
!
!
!
!
interface FastEthernet0/0
 ip address dhcp
 duplex auto
 speed auto
!
interface FastEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface FastEthernet1/0
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface FastEthernet1/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
no ip http server
no ip http secure-server
!
!
!
ip access-list standard ACL_telnet_ssh_snmp
 remark extern 1
 permit 195.20.133.6
 remark extern 2
 permit 212.202.166.58
 remark Eschborner Ldstr 1
 permit 192.168.88.0 0.0.0.255
 remark Eschborner Ldstr 2
 permit 172.23.210.0 0.0.0.255
 remark Interxion
 permit 88.205.102.128 0.0.0.127
 remark Initial Netz
 permit 192.1.1.0 0.0.0.255
!
logging history informational
logging alarm informational
logging trap errors
logging facility local1
logging 10.101.2.113
snmp-server community bross RO ACL_telnet_ssh_snmp
snmp-server community 5NMP-Wr1t3-(0mm RW ACL_telnet_ssh_snmp
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
gatekeeper
 shutdown
!
!
line con 0
 login local
 stopbits 1
line aux 0
 login local
 stopbits 1
line vty 0 4
 session-timeout 60 
 access-class ACL_telnet_ssh_snmp in
 exec-timeout 60 0
 login local
 transport input all
!
ntp server 90.200.31.23
ntp server 90.200.31.21 prefer
!
end
